Exercises

1. Which modules generate the IRQ0, IRQ10 and IRQ16 interrupt requests? Examine the Interrupt Vector Assignments table in the reference manual and the appropriate *device*.h file.

IRQ0: GPIO Interrupt on Port 0.

IRQ10: SCB1 (Serial Communication Block 1).

IRQ16: TCPWM0 (Timer/Counter/PWM 0).

The next several questions involve configuring registers so that if interrupts IRQ0, IRQ10 and IRQ16 are requested simultaneously, the CPU responds as requested. For each question, explain what values must be loaded into which registers, and then write C code which uses the CMSIS functions to perform that operation.

1. Interrupts are serviced in order IRQ10, IRQ0, IRQ16.

Priorities must be in increasing in the above order. For example, 1, 2, 3, or 0, 1, 2.

NVIC\_SetPriority(IRQ10, 1);

NVIC\_SetPriority(IRQ0, 2);

NVIC\_SetPriority(IRQ16, 3);

1. Interrupts are serviced in order IRQ0, IRQ16, IRQ10.

Priorities must be in increasing in the above order. For example, 1, 2, 3, or 0, 1, 2.

NVIC\_SetPriority(IRQ0, 0);

NVIC\_SetPriority(IRQ16, 1);

NVIC\_SetPriority(IRQ10, 2);

1. No interrupts are serviced.

Set PRIMASK to 1.

\_\_disable\_irq();

1. We wish to enable IRQ13 but disable IRQ24. What value needs to be loaded into which register bits, and what is the CMSIS code call to accomplish the same?

Set NVIC\_ISER[13] to 1

NVIC\_EnableIRQ(IRQ13);

Set NVIC\_ICER[24] to 1

NVIC\_DisableIRQ(IRQ24);

1. We wish to determine if IRQ7 has been requested. Which register and which bit will indicate this? What is the CMSIS call which will reveal the information?

Read bit 7 of either NVIC\_ISPR or NVIC\_ICPR

n = NVIC\_GetPendingIRQ(IRQ7);

1. Which register can an exception handler use to determine if it is servicing exception number 0x21? What value will the register have? What is the CMSIS interface code to read the IPSR?

Examine IPSR (or xPSR); the 6 LSBs hold the exception number (0x21).

Get\_IPSR();

1. Fill in the table below to show the contents of memory and registers after the CPU responds to an IRQ2 exception request but before it executes the first instruction of the exception handler.

Initial State:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Register** | **Value** | **Register** | **Value** | **Register/State** | **Value** |
| R0 | 10 | R8 | 18 | xPSR | 0x0100\_0000 |
| R1 | 11 | R9 | 19 | MSP | 0x2000\_0FF4 |
| R2 | 12 | R10 | 20 | PSP | n/a |
| R3 | 13 | R11 | 21 | PRIMASK | 0x0000\_0000 |
| R4 | 14 | R12 | 22 |  |  |
| R5 | 15 | R13 (SP) | 0x2000\_0FF4 | Mode | Thread |
| R6 | 16 | R14 (LR) | 0x1000\_0000 | Privilege | Privileged |
| R7 | 17 | R15 (PC) | 0x0000\_0220 | Stack | Main |

|  |  |
| --- | --- |
| **Exception No.** | **Value** |
| 12 | 0x0000\_1441 |
| 13 | 0x0000\_1211 |
| 14 | 0x0000\_1335 |
| 15 | 0x0000\_1669 |
| 16 | 0x0000\_120D |
| 17 | 0x0000\_1129 |
| 18 | 0x0000\_1351 |
| 19 | 0x0000\_1539 |
| 20 | 0x0000\_1285 |
| 21 | 0x0000\_183D |
| 22 | 0x0000\_1849 |
| 23 | 0x0000\_1661 |

After responding to exception request, before executing exception handler:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Register** | **Value** | **Register** | **Value** | **Register/State** | **Value** |
| R0 | 10 | R8 | 18 | xPSR | 0x0100\_0012 |
| R1 | 11 | R9 | 19 | MSP | 0x2000\_0FD4 |
| R2 | 12 | R10 | 20 | PSP | n/a |
| R3 | 13 | R11 | 21 | PRIMASK | 0x0000\_0000 |
| R4 | 14 | R12 | 22 |  |  |
| R5 | 15 | R13 (SP) | 0x2000\_0FD4 | Mode | Handler |
| R6 | 16 | R14 (LR) | 0xFFFF\_FFF9 | Privilege | Privileged |
| R7 | 17 | R15 (PC) | 0x0000\_1351 | Stack | Main |

|  |  |  |
| --- | --- | --- |
| **Address** | **Value** | **Description** |
| 0x2000\_0FD4 | 10 | R0 |
| 0x2000\_0FD8 | 11 | R1 |
| 0x2000\_0FDC | 12 | R2 |
| 0x2000\_0FE0 | 13 | R3 |
| 0x2000\_0FE4 | 22 | R12 |
| 0x2000\_0FE8 | 0x1000\_0000 | LR |
| 0x2000\_0FEC | 0x0000\_0220 | PC |
| 0x2000\_0FF0 | 0x0100\_0000 | xPSR |

1. What is the return address will an exception handler return to, given the following register and memory contents? Assume the instruction for exiting the exception handler is POP {R4,PC}.

Graphical user interface, application, table

Description automatically generated with medium confidence

The return address is 0x0000\_0B38, stored at 0x2000\_0FE8.

Consider a system built on a 48MHz processor with a main loop and an interrupt which occurs at a 10kHz frequency. Assume the ISR takes 14.9 us to execute and there is a total of 1 us of response and return time overhead.

1. What percentage of the processor’s time is spent in interrupt response and return overhead?

15.9%

1. What percentage of the processor’s time is left for the main loop to execute?

84.1%

1. If the main loop requires 37ms of computation to execute one iteration, what is the minimum main loop update rate (in Hz)?

22.73Hz

Consider the system above again, but now with the interrupt running at 25kHz and the ISR taking 34 us to execute.

1. What percentage of the processor’s time is spent in interrupt response and return overhead?

87.5%

1. What percentage of the processor’s time is left for the main loop to execute?

12.5%

1. If the main loop requires 37ms of computation to execute one iteration, what is the minimum main loop update rate (in Hz)?

3.38Hz